FASTT Telescope

Instrumentation and Reductions • 20-cm meridian telescope

⇒ 0.9 × 0.9 deg field of view (50 Tycho-2 stars) ⇒ Full or partial TDI scanning • Detector

⇒ Ford/Loral 2048^2 CCD (15¯m pixels) ⇒ Anti-blooming logic for bright objects • All reductions make differentially to Tycho-2 ⇒ Positional accuracy ∼ ±60 mas ⇒ Photometric ∼ ±0.03 mag Operation

• All aspects (target selection → observations → reductions → final positions) are fully automated • Rapid processing and publishing of data