New USNOFS 1.3m Astrometric Reflector

• Field of view = 1.3 degree across • Tiled focal plane

⇒ 2 × 3 CCD array ⇒ 2048 × 4096 SITE thinned CCDs • UBVRI and wide-R filters • Fully automated